|ONBOOT="yes"
IFACE="eth0"
SERVICE="dhclient"
DHCP_START=""
DHCP_STOP=""

# Set PRINTIP="yes" to have the script print
# the DHCP assigned IP address
PRINTIP="no"

# Set PRINTALL="yes" to print the DHCP assigned values for
# IP, SM, DG, and 1st NS. This requires PRINTIP="yes".
PRINTALL="no"|
